[Return to first page]
1. Device drivers installation

To install the device drivers, please follow the instructions in the separate Installation Manual.
[Caution]

- The KN2600/2400 may not operate correctly if you install the device drivers using a procedure other than the one described in the installation manual.

- Please wait at least 10 seconds after turning off the KN2600/2400 power before turning it on again, or after unplugging the USB cable before plugging it in again.

- Please exit the application before turning off the KN2600/2400 power or unplugging the USB cable.

- With Windows XP, the screen below (Screen 1) may appear, but you can continue the installation with no problem. Push [Continue Anyway] button and continue the installation.

  (This screen is appeared because the Panasonic USB MIDI driver does not get the Microsoft WHQL - Windows Logo.)

  (Screen 1)

- In upgrading Windows from Windows 98/Me to Windows2000/XP, follow the steps below.
  1. Uninstall the Device Drivers for KN2600/2400 and the application.
  2. Upgrade Windows from Windows 98/Me to Windows 2000/XP.
  3. Install the Device Drivers and the application for Windows 2000/XP.

Device driver limitations

- About the Standby and Hibernate mode (Windows® 98/Me)
  The drivers do not support the Standby and Hibernate mode, and these modes are not available when the KN2600/2400 is connected to your computer.
  If you attempt to activate the Standby or Hibernate mode, the following dialog box appears.
  - Windows® 98
  - Windows® Me
  To put your computer in the Standby or Hibernate mode, turn off the power to the KN2600/2400, or unplug the USB cable connecting the KN2600/2400 to your computer.

[Return to first page]

* Windows is a registered trademark of Microsoft Corporation in the United States and/or other countries.